(export (version D)
  (design
    (source F:\kicad-launchpad\git_testing\demos\kit-dev-coldfire-xilinx_5213\kit-dev-coldfire-xilinx_5213.sch)
    (date "06/05/2018 11:21:35")
    (tool "Eeschema (5.0.0-rc2-dev-665-g57f4903-dirty)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Dev kit coldfire 5213")
        (company)
        (rev 0)
        (date "Sun 22 Mar 2015")
        (source kit-dev-coldfire-xilinx_5213.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /inout_user/) (tstamps /47D80202/)
      (title_block
        (title "Dev kit coldfire 5213")
        (company)
        (rev 0)
        (date "Sun 22 Mar 2015")
        (source in_out_conn.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /xilinx/) (tstamps /47D80204/)
      (title_block
        (title "Dev kit coldfire 5213")
        (company)
        (rev 0)
        (date "Sun 22 Mar 2015")
        (source xilinx.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value MCF5213-LQFP100)
      (footprint Package_QFP:LQFP-100_14x14mm_P0.5mm)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part MCF5213-LQFP100))
      (sheetpath (names /) (tstamps /))
      (tstamp 46161C39))
    (comp (ref C18)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46238286))
    (comp (ref GND1)
      (value CONN_1)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 465FE6C5))
    (comp (ref U2)
      (value 74AHC1G14)
      (footprint lib_smd:SOT353)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part 74AHC1G14))
      (sheetpath (names /) (tstamps /))
      (tstamp 46554FB5))
    (comp (ref CT1)
      (value JUMPER)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 46545507))
    (comp (ref RST_SW1)
      (value SW_PUSH)
      (footprint discret:SW_PUSH_SMALL)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 465451D4))
    (comp (ref Y1)
      (value 8MHz)
      (footprint Crystal:Crystal_HC18-U_Horizontal)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CRYSTAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 462389C7))
    (comp (ref C2)
      (value 10pF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 462389C0))
    (comp (ref C1)
      (value 10pF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 462389BC))
    (comp (ref R1)
      (value 1M)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 462389B6))
    (comp (ref ALLPST1)
      (value CONN_1)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 46238965))
    (comp (ref RED1)
      (value LED_RESET1)
      (footprint lib_smd:SM1206POL)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 46238597))
    (comp (ref R22)
      (value 270)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4623857F))
    (comp (ref R21)
      (value 4.7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 46238545))
    (comp (ref Q1)
      (value 3906)
      (footprint lib_smd:SOT23EBC)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part PNP))
      (sheetpath (names /) (tstamps /))
      (tstamp 46238519))
    (comp (ref R15)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4623847B))
    (comp (ref D3)
      (value BAT54)
      (footprint Diode_SMD:D_SOT-23_ANK)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 4623846D))
    (comp (ref C3)
      (value 1nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46238468))
    (comp (ref LV1)
      (value DS1818)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part MC34064P))
      (sheetpath (names /) (tstamps /))
      (tstamp 462383E5))
    (comp (ref C16)
      (value 10uF)
      (footprint lib_smd:SM1206POL)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 462382CE))
    (comp (ref FB1)
      (value BEAD)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.24x1.80mm_HandSolder)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 462380B8))
    (comp (ref L1)
      (value 10uH)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.24x1.80mm_HandSolder)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 46238092))
    (comp (ref VDDA1)
      (value JUMPER)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 46238079))
    (comp (ref D1)
      (value BAT54)
      (footprint Diode_SMD:D_SOT-23_ANK)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 46237F86))
    (comp (ref ABRT_SW1)
      (value SW_PUSH)
      (footprint discret:SW_PUSH_SMALL)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 46237F50))
    (comp (ref LEDABRT1)
      (value RED)
      (footprint lib_smd:SM1206POL)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 46237E52))
    (comp (ref R14)
      (value 270)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 46237E3D))
    (comp (ref C15)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46237E36))
    (comp (ref R12)
      (value 20K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 46237E2F))
    (comp (ref R7)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 46237E28))
    (comp (ref C14)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46237DF9))
    (comp (ref R45)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE50C))
    (comp (ref C20)
      (value 1nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE364))
    (comp (ref C21)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE35C))
    (comp (ref L2)
      (value 10uH)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.24x1.80mm_HandSolder)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE327))
    (comp (ref R9)
      (value 0)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE230))
    (comp (ref R13)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE054))
    (comp (ref R11)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE051))
    (comp (ref R10)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE04B))
    (comp (ref R8)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE047))
    (comp (ref R6)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE046))
    (comp (ref R5)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE041))
    (comp (ref R4)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BE039))
    (comp (ref TA-1)
      (value CONN_1)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BBA34))
    (comp (ref R26)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB8C0))
    (comp (ref CLKOUT1)
      (value CONN_1)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB894))
    (comp (ref R20)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB799))
    (comp (ref R19)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB798))
    (comp (ref R18)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB795))
    (comp (ref R17)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB790))
    (comp (ref R46)
      (value 22)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB742))
    (comp (ref R2)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB661))
    (comp (ref R25)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB65F))
    (comp (ref CLK1)
      (value JUMPER)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB648))
    (comp (ref CLK0)
      (value JUMPER)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB62E))
    (comp (ref C6)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BB5E5))
    (comp (ref R16)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BAF5C))
    (comp (ref BDM_EN1)
      (value JUMPER)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BAF4F))
    (comp (ref BDM_PORT1)
      (value CONN_13X2)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x13_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_13X2))
      (sheetpath (names /) (tstamps /))
      (tstamp 461BAEE7))
    (comp (ref C17)
      (value 100uF)
      (footprint lib_smd:SM1206POL)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 46161D3C))
    (comp (ref C12)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46161CDA))
    (comp (ref C11)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46161CD9))
    (comp (ref C10)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46161CD8))
    (comp (ref C9)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46161CD7))
    (comp (ref C8)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46161CD4))
    (comp (ref C7)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46161CD3))
    (comp (ref C5)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46161CB8))
    (comp (ref C4)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 46161CB5))
    (comp (ref VR1)
      (value LT1129_QPACK)
      (footprint Package_TO_SOT_SMD:TO-263-5_TabPin3)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part LT1129_QPACK))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 46603376))
    (comp (ref C26)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 46546CA6))
    (comp (ref RCAN1)
      (value R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4654018B))
    (comp (ref RCAN2)
      (value R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 46540184))
    (comp (ref R38)
      (value 62)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 46540164))
    (comp (ref CAN_TERM1)
      (value JUMPER)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part JUMPER))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 46540159))
    (comp (ref RS1)
      (value CONN_1)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_1))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4654007F))
    (comp (ref R36)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 46540063))
    (comp (ref VREF1)
      (value CONN_1)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_1))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4654003D))
    (comp (ref C34)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4653FFFE))
    (comp (ref U7)
      (value PCA82C251)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part PCA82C251))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4653FF97))
    (comp (ref TB1)
      (value CONN_2)
      (footprint connect:bornier2)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_2))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 46530806))
    (comp (ref J1)
      (value JACK_2P)
      (footprint connect:JACK_ALIM)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part JACK_2P))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 465307C6))
    (comp (ref SW_ONOFF1)
      (value SWITCH_INV)
      (footprint discret:SW_SPDT)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part SWITCH_INV))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 46530763))
    (comp (ref F1)
      (value FUSE)
      (footprint lib_smd:FSUPCMS)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part FUSE))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 46530747))
    (comp (ref C41)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 465306F6))
    (comp (ref D7)
      (value 1N4004)
      (footprint Diode_THT:D_DO-15_P12.70mm_Horizontal)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part DIODE))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 465306C8))
    (comp (ref C38)
      (value 10uF)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CP))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 465306B1))
    (comp (ref LED5)
      (value LED)
      (footprint LED_SMD:LED_1206_3216Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part LED))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 46530639))
    (comp (ref R53)
      (value 270)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 46530638))
    (comp (ref C40)
      (value 220uF)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CP))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 465305FE))
    (comp (ref SW2)
      (value SW_PUSH)
      (footprint discret:SW_PUSH_SMALL)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part SW_PUSH))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652DDE7))
    (comp (ref SW1)
      (value SW_PUSH)
      (footprint discret:SW_PUSH_SMALL)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part SW_PUSH))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652DDDF))
    (comp (ref CAN_EN1)
      (value CONN_2X2)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_2X2))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652BFF1))
    (comp (ref R47)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652BF65))
    (comp (ref R48)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652BF62))
    (comp (ref R49)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652BF5C))
    (comp (ref R50)
      (value 4,7K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652BF48))
    (comp (ref PULUPEN1)
      (value CONN_4X2)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_4X2))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652BF26))
    (comp (ref COM_SEL1)
      (value CONN_3)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_3))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652BADD))
    (comp (ref COM_SEL2)
      (value CONN_3)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_3))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652BAD4))
    (comp (ref COM_SEL3)
      (value CONN_3)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_3))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652BA65))
    (comp (ref R30)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B9D5))
    (comp (ref R35)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B9CC))
    (comp (ref R23)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B5F4))
    (comp (ref C45)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4DC))
    (comp (ref C46)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4D9))
    (comp (ref C36)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4D8))
    (comp (ref C44)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4D7))
    (comp (ref C35)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4D6))
    (comp (ref UART_EN2)
      (value CONN_4X2)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_4X2))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4D5))
    (comp (ref UARTCAN2)
      (value DB9)
      (footprint connect:DB9FC)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part DB9))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4D4))
    (comp (ref U8)
      (value MAX202)
      (footprint Package_SO:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part MAX202))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4D3))
    (comp (ref C33)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4CA))
    (comp (ref C28)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4C7))
    (comp (ref C32)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4C6))
    (comp (ref C31)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4C5))
    (comp (ref C30)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4C4))
    (comp (ref UART_EN1)
      (value CONN_4X2)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_4X2))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4C3))
    (comp (ref UARTCAN1)
      (value DB9)
      (footprint connect:DB9FC)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part DB9))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4C2))
    (comp (ref U5)
      (value MAX202)
      (footprint Package_SO:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part MAX202))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B4C1))
    (comp (ref C27)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B486))
    (comp (ref C22)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B365))
    (comp (ref C25)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B35B))
    (comp (ref C24)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B354))
    (comp (ref C23)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B33B))
    (comp (ref UART_EN0)
      (value CONN_4X2)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_4X2))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B289))
    (comp (ref UARTCAN0)
      (value DB9)
      (footprint connect:DB9FC)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part DB9))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B26D))
    (comp (ref U3)
      (value MAX202)
      (footprint Package_SO:SOIC-16_3.9x9.9mm_P1.27mm)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part MAX202))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B22B))
    (comp (ref R34)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B111))
    (comp (ref LED_EN1)
      (value JUMPER)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part JUMPER))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B108))
    (comp (ref LED4)
      (value LED)
      (footprint LED_SMD:LED_1206_3216Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part LED))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B0BC))
    (comp (ref LED3)
      (value LED)
      (footprint LED_SMD:LED_1206_3216Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part LED))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B0BB))
    (comp (ref LED2)
      (value LED)
      (footprint LED_SMD:LED_1206_3216Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part LED))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B0B7))
    (comp (ref LED1)
      (value LED)
      (footprint LED_SMD:LED_1206_3216Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part LED))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B0AE))
    (comp (ref R33)
      (value 270)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B06A))
    (comp (ref R32)
      (value 270)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B069))
    (comp (ref R31)
      (value 270)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B067))
    (comp (ref R28)
      (value 270)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B061))
    (comp (ref U4)
      (value 74HC125)
      (footprint Package_SO:SOIC-14_3.9x8.7mm_P1.27mm)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part 74LS125))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652B03E))
    (comp (ref C43)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652A9D3))
    (comp (ref VX_EN1)
      (value JUMPER)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part JUMPER))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652A9C4))
    (comp (ref MCU_PORT1)
      (value CONN_30X2)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x30_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_30X2))
      (sheetpath (names /inout_user/) (tstamps /47D80202/))
      (tstamp 4652A4FB))
    (comp (ref R64)
      (value 3,3)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 4791D59D))
    (comp (ref P3)
      (value CONN_2X2)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_2X2))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76EB2))
    (comp (ref U9)
      (value XCR3256-TQ144)
      (footprint Package_QFP:TQFP-144_20x20mm_P0.5mm)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part XCR3256-TQ144))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 470F38BE))
    (comp (ref P4)
      (value CONN_20X2)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_20X2))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46ADE55A))
    (comp (ref R57)
      (value 4K7)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BCA))
    (comp (ref D8)
      (value LED)
      (footprint LED_SMD:LED_1206_3216Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part LED))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BC4))
    (comp (ref R62)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BC3))
    (comp (ref C61)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BBC))
    (comp (ref C60)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BBB))
    (comp (ref C59)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BBA))
    (comp (ref C54)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BB5))
    (comp (ref C53)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BB4))
    (comp (ref C52)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BB3))
    (comp (ref C51)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BB2))
    (comp (ref C58)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BB1))
    (comp (ref C57)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BB0))
    (comp (ref C56)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BAF))
    (comp (ref C55)
      (value 100nF)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part C))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BAE))
    (comp (ref D9)
      (value LED)
      (footprint LED_SMD:LED_1206_3216Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part LED))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BA8))
    (comp (ref R63)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part R))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BA7))
    (comp (ref P1)
      (value CONN_6)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical)
      (libsource (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_6))
      (sheetpath (names /xilinx/) (tstamps /47D80204/))
      (tstamp 46A76BA6)))
  (libparts
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part 74AHC1G14)
      (fields
        (field (name Reference) U)
        (field (name Value) 74AHC1G14))
      (pins
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name ~) (type output))
        (pin (num 5) (name VCC) (type power_in))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part 74LS125)
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS125))
      (pins
        (pin (num 1) (name E) (type input))
        (pin (num 2) (name D) (type input))
        (pin (num 3) (name O) (type 3state))
        (pin (num 4) (name E) (type input))
        (pin (num 5) (name D) (type input))
        (pin (num 6) (name O) (type 3state))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name O) (type 3state))
        (pin (num 9) (name D) (type input))
        (pin (num 10) (name E) (type input))
        (pin (num 11) (name O) (type 3state))
        (pin (num 12) (name D) (type input))
        (pin (num 13) (name E) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part C)
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_1)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_13X2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_13X2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P20) (type passive))
        (pin (num 25) (name P24) (type passive))
        (pin (num 26) (name P22) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_20X2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_20X2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name ~) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))
        (pin (num 40) (name P40) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_2X2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2X2))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_3)
      (fields
        (field (name Reference) K)
        (field (name Value) CONN_3))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_30X2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_30X2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name ~) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))
        (pin (num 40) (name P40) (type passive))
        (pin (num 41) (name P41) (type passive))
        (pin (num 42) (name P42) (type passive))
        (pin (num 43) (name P43) (type passive))
        (pin (num 44) (name P44) (type passive))
        (pin (num 45) (name P45) (type passive))
        (pin (num 46) (name P46) (type passive))
        (pin (num 47) (name P47) (type passive))
        (pin (num 48) (name P48) (type passive))
        (pin (num 49) (name P49) (type passive))
        (pin (num 50) (name P50) (type passive))
        (pin (num 51) (name P51) (type passive))
        (pin (num 52) (name P52) (type passive))
        (pin (num 53) (name P53) (type passive))
        (pin (num 54) (name P54) (type passive))
        (pin (num 55) (name P55) (type passive))
        (pin (num 56) (name P56) (type passive))
        (pin (num 57) (name P57) (type passive))
        (pin (num 58) (name P58) (type passive))
        (pin (num 59) (name P59) (type passive))
        (pin (num 60) (name P60) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_4X2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_4X2))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part CONN_6)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_6))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part CP)
      (aliases
        (alias CAPAPOL))
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part CRYSTAL)
      (fields
        (field (name Reference) X)
        (field (name Value) CRYSTAL))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part DB9)
      (footprints
        (fp DB9*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB9))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part DIODE)
      (description "Diode, alternativ symbol")
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODE))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part FUSE)
      (fields
        (field (name Reference) F)
        (field (name Value) FUSE))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part INDUCTOR)
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part JACK_2P)
      (fields
        (field (name Reference) J)
        (field (name Value) JACK_2P))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part JUMPER)
      (fields
        (field (name Reference) JP)
        (field (name Value) JUMPER))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part LT1129_QPACK)
      (aliases
        (alias LT_1129_QP))
      (fields
        (field (name Reference) U)
        (field (name Value) LT1129_QPACK))
      (pins
        (pin (num 1) (name OUT) (type power_out))
        (pin (num 2) (name SENSE) (type input))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name SHDN) (type input))
        (pin (num 5) (name IN) (type input))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part MAX232)
      (aliases
        (alias MAX202))
      (fields
        (field (name Reference) U)
        (field (name Value) MAX232))
      (pins
        (pin (num 1) (name C1+) (type input))
        (pin (num 2) (name V+) (type power_out))
        (pin (num 3) (name C1-) (type input))
        (pin (num 4) (name C2+) (type input))
        (pin (num 5) (name C2-) (type input))
        (pin (num 6) (name V-) (type power_out))
        (pin (num 7) (name T2OUT) (type output))
        (pin (num 8) (name R2IN) (type input))
        (pin (num 9) (name R2OUT) (type output))
        (pin (num 10) (name T2IN) (type input))
        (pin (num 11) (name T1IN) (type input))
        (pin (num 12) (name R1OUT) (type output))
        (pin (num 13) (name R1IN) (type input))
        (pin (num 14) (name T1OUT) (type output))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part MC34064P)
      (aliases
        (alias MC33064P))
      (fields
        (field (name Reference) U)
        (field (name Value) MC34064P))
      (pins
        (pin (num 1) (name Rst) (type openCol))
        (pin (num 2) (name In) (type input))
        (pin (num 3) (name Gbd) (type input))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part MCF5213-LQFP100)
      (fields
        (field (name Reference) U)
        (field (name Value) MCF5213-LQFP100))
      (pins
        (pin (num 1) (name VCC) (type power_in))
        (pin (num 2) (name VCC) (type power_in))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name ~URTS1~/SYNCB/UTXD2/PUB2) (type BiDi))
        (pin (num 5) (name TEST) (type input))
        (pin (num 6) (name ~UCTS0~/CANRX/PUA3) (type BiDi))
        (pin (num 7) (name URXD0/PUA1) (type BiDi))
        (pin (num 8) (name UTXD0/PUA0) (type BiDi))
        (pin (num 9) (name ~URTS0~/CANTX/PUA2) (type BiDi))
        (pin (num 10) (name SCL/CANTX/PAS0/UTXD2) (type BiDi))
        (pin (num 11) (name SDA/CANRX/PAS1/URXD2) (type BiDi))
        (pin (num 12) (name QSPI_CS3/SYNCA/SYNCB/PQS6) (type BiDi))
        (pin (num 13) (name QSPI_CS2/PQS5) (type BiDi))
        (pin (num 14) (name VCC) (type power_in))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name QSPI_DIN/EZPD/CANRX/RXD1/PQS1) (type BiDi))
        (pin (num 17) (name QSPI_DOUT/EZPQ/CANTX/RXD0/PQS0) (type BiDi))
        (pin (num 18) (name QSPI_CLK/EZPCK/SCL/RTS1/PQS2) (type BiDi))
        (pin (num 19) (name QSPI_CS1/PQS4) (type BiDi))
        (pin (num 20) (name QSPI_CS0/SDA/CTS1/PQS3) (type BiDi))
        (pin (num 21) (name RCON/EZPCS) (type input))
        (pin (num 22) (name VCC) (type power_in))
        (pin (num 23) (name VCC) (type power_in))
        (pin (num 24) (name GND) (type power_in))
        (pin (num 25) (name GND) (type power_in))
        (pin (num 26) (name JTAG_EN) (type input))
        (pin (num 27) (name ~UCTS2~/PUC3) (type BiDi))
        (pin (num 28) (name URXD2/PUC1) (type BiDi))
        (pin (num 29) (name UTXD2/PUC0) (type BiDi))
        (pin (num 30) (name ~URTS2~/PUC2) (type BiDi))
        (pin (num 31) (name DTIN2/DTOUT2/PWM4/PTC2) (type BiDi))
        (pin (num 32) (name DTIN3/DTOUT3/PWM6/PTC3) (type BiDi))
        (pin (num 33) (name PWM3/PTD1) (type BiDi))
        (pin (num 34) (name VCC) (type power_in))
        (pin (num 35) (name GND) (type power_in))
        (pin (num 36) (name DTIN0/DTOUT0/PWM0/PTC0) (type BiDi))
        (pin (num 37) (name DTIN1/DTOUT1/PWM2/PTC1) (type BiDi))
        (pin (num 38) (name PWM1/PTD0) (type BiDi))
        (pin (num 39) (name CLKMOD1) (type input))
        (pin (num 40) (name CLKMOD0) (type input))
        (pin (num 41) (name VCC) (type power_in))
        (pin (num 42) (name GND) (type power_in))
        (pin (num 43) (name AN0/PAN0) (type BiDi))
        (pin (num 44) (name AN1/PAN1) (type BiDi))
        (pin (num 45) (name AN2/PAN2) (type BiDi))
        (pin (num 46) (name AN3/PAN3) (type BiDi))
        (pin (num 47) (name VSSA) (type input))
        (pin (num 48) (name VRL) (type input))
        (pin (num 49) (name VRH) (type input))
        (pin (num 50) (name VCCA) (type input))
        (pin (num 51) (name AN7/PAN7) (type BiDi))
        (pin (num 52) (name AN6/PAN6) (type BiDi))
        (pin (num 53) (name AN5/PAN5) (type BiDi))
        (pin (num 54) (name AN4/PAN4) (type BiDi))
        (pin (num 55) (name VSTBY) (type power_in))
        (pin (num 56) (name GND) (type power_in))
        (pin (num 57) (name VCC) (type power_in))
        (pin (num 58) (name GPT0/PWM1/PTA0) (type BiDi))
        (pin (num 59) (name GPT1/PWM3/PTA1) (type BiDi))
        (pin (num 60) (name PWM5/PTD2) (type BiDi))
        (pin (num 61) (name GPT2PWM5//PTA2) (type BiDi))
        (pin (num 62) (name GPT3/PWM7/PTA3) (type BiDi))
        (pin (num 63) (name PWM7/PTD3) (type BiDi))
        (pin (num 64) (name TCLK/PSTCLK/CLKOUT) (type input))
        (pin (num 65) (name PST0/PDD0) (type BiDi))
        (pin (num 66) (name PST1/PDD1) (type BiDi))
        (pin (num 67) (name GND) (type power_in))
        (pin (num 68) (name VCC) (type power_in))
        (pin (num 69) (name PST2/PDD2) (type BiDi))
        (pin (num 70) (name PST3/PDD3) (type BiDi))
        (pin (num 71) (name GNDPLL) (type passive))
        (pin (num 72) (name XTAL) (type output))
        (pin (num 73) (name CLKIN/EXTAL) (type input))
        (pin (num 74) (name VCCPLL) (type passive))
        (pin (num 75) (name GND) (type power_in))
        (pin (num 76) (name ~BKPT~/TMS) (type input))
        (pin (num 77) (name DDATA0/PDD4) (type BiDi))
        (pin (num 78) (name DDATA1/PDD5) (type BiDi))
        (pin (num 79) (name DSI/TDI) (type input))
        (pin (num 80) (name DSO/TDO) (type output))
        (pin (num 81) (name VCC) (type power_in))
        (pin (num 82) (name GND) (type power_in))
        (pin (num 83) (name DDATA2/PDD6) (type BiDi))
        (pin (num 84) (name DDATA3/PDD7) (type BiDi))
        (pin (num 85) (name DSCLK/~TRST~) (type input))
        (pin (num 86) (name ALLPST) (type output))
        (pin (num 87) (name ~IRQ1~/PNQ1/SYNCA/PWM1) (type BiDi))
        (pin (num 88) (name ~IRQ2~/PNQ2) (type BiDi))
        (pin (num 89) (name ~IRQ3~/PNQ3) (type BiDi))
        (pin (num 90) (name ~IRQ4~/PNQ4) (type BiDi))
        (pin (num 91) (name ~IRQ5~/PNQ5) (type BiDi))
        (pin (num 92) (name GND) (type power_in))
        (pin (num 93) (name VCC) (type power_in))
        (pin (num 94) (name ~IRQ6~/PNQ6) (type BiDi))
        (pin (num 95) (name ~IRQ7~/PNQ7) (type BiDi))
        (pin (num 96) (name RSTI) (type input))
        (pin (num 97) (name RSTO) (type output))
        (pin (num 98) (name ~UCTS1~/SYNCA/URXD2/PUB3) (type BiDi))
        (pin (num 99) (name UTXD1/PUB0) (type BiDi))
        (pin (num 100) (name URXD1/PUB1) (type BiDi))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part PCA82C251)
      (fields
        (field (name Reference) U)
        (field (name Value) PCA82C251))
      (pins
        (pin (num 1) (name TxD) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name VCC) (type power_in))
        (pin (num 4) (name RxD) (type output))
        (pin (num 5) (name Vref) (type output))
        (pin (num 6) (name CAN-) (type BiDi))
        (pin (num 7) (name CAN+) (type BiDi))
        (pin (num 8) (name Rsl) (type input))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part PNP)
      (fields
        (field (name Reference) Q)
        (field (name Value) PNP))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part R)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part SWITCH_INV)
      (fields
        (field (name Reference) SW)
        (field (name Value) SWITCH_INV))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part SW_PUSH)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib kit-dev-coldfire-xilinx_5213_schlib) (part XCR3256-TQ144)
      (fields
        (field (name Reference) U)
        (field (name Value) XCR3256-TQ144))
      (pins
        (pin (num 1) (name I1) (type passive))
        (pin (num 2) (name I0) (type passive))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name J0/TDI) (type passive))
        (pin (num 5) (name J2) (type passive))
        (pin (num 6) (name J3) (type passive))
        (pin (num 7) (name J4) (type passive))
        (pin (num 8) (name J11) (type passive))
        (pin (num 9) (name J13) (type passive))
        (pin (num 10) (name J14) (type passive))
        (pin (num 11) (name J15) (type passive))
        (pin (num 12) (name L2) (type passive))
        (pin (num 13) (name PORT_EN) (type passive))
        (pin (num 14) (name L3) (type passive))
        (pin (num 15) (name L4) (type passive))
        (pin (num 16) (name L11) (type passive))
        (pin (num 17) (name GND) (type power_in))
        (pin (num 18) (name L13) (type passive))
        (pin (num 19) (name L14) (type passive))
        (pin (num 20) (name N0/TMS) (type passive))
        (pin (num 21) (name N2) (type passive))
        (pin (num 22) (name N3) (type passive))
        (pin (num 23) (name N4) (type passive))
        (pin (num 24) (name VCC) (type power_in))
        (pin (num 25) (name N11) (type passive))
        (pin (num 26) (name N13) (type passive))
        (pin (num 27) (name N14) (type passive))
        (pin (num 28) (name N15) (type passive))
        (pin (num 29) (name P2) (type passive))
        (pin (num 30) (name P3) (type passive))
        (pin (num 31) (name P4) (type passive))
        (pin (num 32) (name P11) (type passive))
        (pin (num 33) (name GND) (type power_in))
        (pin (num 34) (name P13) (type passive))
        (pin (num 35) (name P14) (type passive))
        (pin (num 36) (name P15) (type passive))
        (pin (num 37) (name O15) (type passive))
        (pin (num 38) (name O13) (type passive))
        (pin (num 39) (name O12) (type passive))
        (pin (num 40) (name O4) (type passive))
        (pin (num 41) (name O3) (type passive))
        (pin (num 42) (name O2) (type passive))
        (pin (num 43) (name O1) (type passive))
        (pin (num 44) (name O0) (type passive))
        (pin (num 45) (name M15) (type passive))
        (pin (num 46) (name M13) (type passive))
        (pin (num 47) (name M12) (type passive))
        (pin (num 48) (name M11) (type passive))
        (pin (num 49) (name M4) (type passive))
        (pin (num 50) (name VCC) (type power_in))
        (pin (num 51) (name VCC) (type power_in))
        (pin (num 52) (name GND) (type power_in))
        (pin (num 53) (name M2) (type passive))
        (pin (num 54) (name M1) (type passive))
        (pin (num 55) (name F1) (type passive))
        (pin (num 56) (name F2) (type passive))
        (pin (num 57) (name GND) (type power_in))
        (pin (num 58) (name VCC) (type power_in))
        (pin (num 59) (name GND) (type power_in))
        (pin (num 60) (name F4) (type passive))
        (pin (num 61) (name F11) (type passive))
        (pin (num 62) (name F12) (type passive))
        (pin (num 63) (name F13) (type passive))
        (pin (num 64) (name GND) (type power_in))
        (pin (num 65) (name F15) (type passive))
        (pin (num 66) (name H0) (type passive))
        (pin (num 67) (name H1) (type passive))
        (pin (num 68) (name H2) (type passive))
        (pin (num 69) (name H3) (type passive))
        (pin (num 70) (name H11) (type passive))
        (pin (num 71) (name H13) (type passive))
        (pin (num 72) (name H15) (type passive))
        (pin (num 73) (name VCC) (type power_in))
        (pin (num 74) (name G14) (type passive))
        (pin (num 75) (name G13) (type passive))
        (pin (num 76) (name VCC) (type power_in))
        (pin (num 77) (name G11) (type passive))
        (pin (num 78) (name G4) (type passive))
        (pin (num 79) (name G3) (type passive))
        (pin (num 80) (name G2) (type passive))
        (pin (num 81) (name G0) (type input))
        (pin (num 82) (name E14) (type passive))
        (pin (num 83) (name E13) (type passive))
        (pin (num 84) (name E11) (type passive))
        (pin (num 85) (name GND) (type power_in))
        (pin (num 86) (name E4) (type passive))
        (pin (num 87) (name E3) (type passive))
        (pin (num 88) (name E2) (type passive))
        (pin (num 89) (name E0/TCK) (type passive))
        (pin (num 90) (name C14) (type passive))
        (pin (num 91) (name C13) (type passive))
        (pin (num 92) (name C11) (type passive))
        (pin (num 93) (name C4) (type passive))
        (pin (num 94) (name C3) (type passive))
        (pin (num 95) (name VCC) (type power_in))
        (pin (num 96) (name C2) (type passive))
        (pin (num 97) (name C1) (type passive))
        (pin (num 98) (name C0) (type passive))
        (pin (num 99) (name A13) (type passive))
        (pin (num 100) (name A12) (type passive))
        (pin (num 101) (name A11) (type passive))
        (pin (num 102) (name A4) (type passive))
        (pin (num 103) (name A3) (type passive))
        (pin (num 104) (name A2/TDO) (type passive))
        (pin (num 105) (name GND) (type power_in))
        (pin (num 106) (name A0) (type passive))
        (pin (num 107) (name B0) (type passive))
        (pin (num 108) (name B1) (type passive))
        (pin (num 109) (name B4) (type passive))
        (pin (num 110) (name B11) (type passive))
        (pin (num 111) (name B12) (type passive))
        (pin (num 112) (name B14) (type passive))
        (pin (num 113) (name B15) (type passive))
        (pin (num 114) (name D0) (type passive))
        (pin (num 115) (name VCC) (type power_in))
        (pin (num 116) (name D1) (type passive))
        (pin (num 117) (name D2) (type passive))
        (pin (num 118) (name D4) (type passive))
        (pin (num 119) (name D11) (type passive))
        (pin (num 120) (name D12) (type passive))
        (pin (num 121) (name D13) (type passive))
        (pin (num 122) (name D15) (type passive))
        (pin (num 123) (name VCC) (type power_in))
        (pin (num 124) (name GND) (type power_in))
        (pin (num 125) (name CLK3/IN3) (type input))
        (pin (num 126) (name CLK2/IN2) (type input))
        (pin (num 127) (name CLK1/IN1) (type input))
        (pin (num 128) (name CLK0/IN0) (type input))
        (pin (num 129) (name GND) (type power_in))
        (pin (num 130) (name VCC) (type power_in))
        (pin (num 131) (name K15) (type passive))
        (pin (num 132) (name K14) (type passive))
        (pin (num 133) (name K13) (type passive))
        (pin (num 134) (name K12) (type passive))
        (pin (num 135) (name GND) (type power_in))
        (pin (num 136) (name K11) (type passive))
        (pin (num 137) (name K4) (type passive))
        (pin (num 138) (name K2) (type passive))
        (pin (num 139) (name I15) (type passive))
        (pin (num 140) (name I14) (type passive))
        (pin (num 141) (name I13) (type passive))
        (pin (num 142) (name I12) (type passive))
        (pin (num 143) (name I4) (type passive))
        (pin (num 144) (name VCC) (type power_in)))))
  (libraries
    (library (logical kit-dev-coldfire-xilinx_5213_schlib)
      (uri F:\kicad-launchpad\git_testing\demos\kit-dev-coldfire-xilinx_5213/kit-dev-coldfire-xilinx_5213_schlib.lib)))
  (nets
    (net (code 1) (name "Net-(LEDABRT1-Pad2)")
      (node (ref R14) (pin 1))
      (node (ref LEDABRT1) (pin 2)))
    (net (code 2) (name GND)
      (node (ref R26) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref U1) (pin 82))
      (node (ref C27) (pin 2))
      (node (ref U5) (pin 15))
      (node (ref UARTCAN0) (pin 5))
      (node (ref C22) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref U4) (pin 7))
      (node (ref U4) (pin 7))
      (node (ref LED_EN1) (pin 1))
      (node (ref C8) (pin 2))
      (node (ref U1) (pin 35))
      (node (ref UARTCAN1) (pin 5))
      (node (ref U1) (pin 42))
      (node (ref U1) (pin 56))
      (node (ref C33) (pin 2))
      (node (ref U1) (pin 25))
      (node (ref U1) (pin 24))
      (node (ref U1) (pin 3))
      (node (ref U1) (pin 15))
      (node (ref C55) (pin 2))
      (node (ref D9) (pin 2))
      (node (ref C58) (pin 2))
      (node (ref C57) (pin 2))
      (node (ref C59) (pin 2))
      (node (ref C56) (pin 2))
      (node (ref P1) (pin 2))
      (node (ref C53) (pin 2))
      (node (ref C61) (pin 2))
      (node (ref C60) (pin 2))
      (node (ref C54) (pin 2))
      (node (ref C52) (pin 2))
      (node (ref C51) (pin 2))
      (node (ref U9) (pin 33))
      (node (ref BDM_PORT1) (pin 11))
      (node (ref BDM_PORT1) (pin 5))
      (node (ref U2) (pin 3))
      (node (ref U1) (pin 92))
      (node (ref C17) (pin 2))
      (node (ref RST_SW1) (pin 2))
      (node (ref CLK0) (pin 1))
      (node (ref U9) (pin 52))
      (node (ref U1) (pin 67))
      (node (ref U9) (pin 57))
      (node (ref U1) (pin 71))
      (node (ref U1) (pin 75))
      (node (ref BDM_PORT1) (pin 23))
      (node (ref CLK1) (pin 1))
      (node (ref P4) (pin 40))
      (node (ref BDM_PORT1) (pin 20))
      (node (ref U9) (pin 3))
      (node (ref BDM_PORT1) (pin 3))
      (node (ref D8) (pin 2))
      (node (ref U9) (pin 59))
      (node (ref U9) (pin 64))
      (node (ref C6) (pin 2))
      (node (ref P4) (pin 2))
      (node (ref GND1) (pin 1))
      (node (ref U9) (pin 85))
      (node (ref BDM_EN1) (pin 1))
      (node (ref U9) (pin 129))
      (node (ref U9) (pin 13))
      (node (ref R12) (pin 2))
      (node (ref R35) (pin 1))
      (node (ref C34) (pin 2))
      (node (ref RED1) (pin 2))
      (node (ref D7) (pin 2))
      (node (ref MCU_PORT1) (pin 54))
      (node (ref C14) (pin 1))
      (node (ref MCU_PORT1) (pin 60))
      (node (ref UARTCAN2) (pin 5))
      (node (ref MCU_PORT1) (pin 3))
      (node (ref U9) (pin 126))
      (node (ref U9) (pin 127))
      (node (ref C26) (pin 2))
      (node (ref U7) (pin 2))
      (node (ref VR1) (pin 3))
      (node (ref FB1) (pin 1))
      (node (ref C45) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref C20) (pin 2))
      (node (ref U9) (pin 135))
      (node (ref U8) (pin 15))
      (node (ref LV1) (pin 3))
      (node (ref R23) (pin 1))
      (node (ref TB1) (pin 2))
      (node (ref C41) (pin 2))
      (node (ref J1) (pin 1))
      (node (ref C15) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref U4) (pin 7))
      (node (ref U3) (pin 15))
      (node (ref R9) (pin 2))
      (node (ref C38) (pin 2))
      (node (ref U4) (pin 7))
      (node (ref U9) (pin 124))
      (node (ref LED1) (pin 2))
      (node (ref LED2) (pin 2))
      (node (ref LED3) (pin 2))
      (node (ref LED4) (pin 2))
      (node (ref R30) (pin 1))
      (node (ref SW1) (pin 2))
      (node (ref C46) (pin 2))
      (node (ref C40) (pin 2))
      (node (ref LED5) (pin 2))
      (node (ref C43) (pin 1))
      (node (ref SW2) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref COM_SEL2) (pin 1))
      (node (ref R36) (pin 2))
      (node (ref U9) (pin 125))
      (node (ref C1) (pin 2))
      (node (ref U9) (pin 105))
      (node (ref U9) (pin 17))
      (node (ref RCAN2) (pin 1))
      (node (ref C3) (pin 2)))
    (net (code 3) (name +3.3V)
      (node (ref C35) (pin 1))
      (node (ref C46) (pin 1))
      (node (ref C56) (pin 1))
      (node (ref C53) (pin 1))
      (node (ref C52) (pin 1))
      (node (ref C51) (pin 1))
      (node (ref C58) (pin 1))
      (node (ref C57) (pin 1))
      (node (ref C54) (pin 1))
      (node (ref C55) (pin 1))
      (node (ref R50) (pin 1))
      (node (ref R49) (pin 1))
      (node (ref R48) (pin 1))
      (node (ref R47) (pin 1))
      (node (ref P1) (pin 1))
      (node (ref C61) (pin 1))
      (node (ref C60) (pin 1))
      (node (ref C59) (pin 1))
      (node (ref U1) (pin 34))
      (node (ref C30) (pin 1))
      (node (ref U1) (pin 41))
      (node (ref C40) (pin 1))
      (node (ref R53) (pin 2))
      (node (ref VX_EN1) (pin 1))
      (node (ref MCU_PORT1) (pin 59))
      (node (ref C28) (pin 1))
      (node (ref C23) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref U5) (pin 16))
      (node (ref U3) (pin 16))
      (node (ref R34) (pin 1))
      (node (ref U4) (pin 14))
      (node (ref U4) (pin 14))
      (node (ref U8) (pin 16))
      (node (ref U4) (pin 14))
      (node (ref U4) (pin 14))
      (node (ref U7) (pin 3))
      (node (ref U1) (pin 2))
      (node (ref U1) (pin 22))
      (node (ref U1) (pin 23))
      (node (ref U1) (pin 1))
      (node (ref U1) (pin 14))
      (node (ref U1) (pin 57))
      (node (ref U1) (pin 55))
      (node (ref U2) (pin 5))
      (node (ref U9) (pin 58))
      (node (ref C34) (pin 1))
      (node (ref U9) (pin 76))
      (node (ref U1) (pin 93))
      (node (ref U9) (pin 73))
      (node (ref RCAN1) (pin 1))
      (node (ref U9) (pin 50))
      (node (ref C22) (pin 1))
      (node (ref U9) (pin 95))
      (node (ref U9) (pin 51))
      (node (ref U1) (pin 81))
      (node (ref U1) (pin 68))
      (node (ref VR1) (pin 2))
      (node (ref VR1) (pin 1))
      (node (ref R13) (pin 2))
      (node (ref R64) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref R17) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref R19) (pin 1))
      (node (ref R20) (pin 1))
      (node (ref L2) (pin 1))
      (node (ref BDM_PORT1) (pin 9))
      (node (ref C17) (pin 1))
      (node (ref R57) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref LV1) (pin 2))
      (node (ref R25) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref VDDA1) (pin 1))
      (node (ref BDM_PORT1) (pin 25))
      (node (ref R15) (pin 1))
      (node (ref U9) (pin 144))
      (node (ref C4) (pin 1))
      (node (ref R5) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref Q1) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref U9) (pin 123))
      (node (ref C10) (pin 1))
      (node (ref U9) (pin 115))
      (node (ref U9) (pin 130))
      (node (ref C11) (pin 1))
      (node (ref U9) (pin 24))
      (node (ref R45) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref ABRT_SW1) (pin 2))
      (node (ref LEDABRT1) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref R16) (pin 1)))
    (net (code 4) (name "Net-(D1-Pad1)")
      (node (ref D1) (pin 1))
      (node (ref R14) (pin 2))
      (node (ref U2) (pin 4)))
    (net (code 5) (name "Net-(ABRT_SW1-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref ABRT_SW1) (pin 1)))
    (net (code 6) (name /QSPI_CS1)
      (node (ref MCU_PORT1) (pin 25))
      (node (ref U9) (pin 54))
      (node (ref U1) (pin 19)))
    (net (code 7) (name /QSPI_DIN)
      (node (ref U9) (pin 46))
      (node (ref U1) (pin 16))
      (node (ref MCU_PORT1) (pin 19)))
    (net (code 8) (name /DSPI_DOUT)
      (node (ref U1) (pin 17))
      (node (ref MCU_PORT1) (pin 17))
      (node (ref U9) (pin 47)))
    (net (code 9) (name /QSPI_CLK)
      (node (ref PULUPEN1) (pin 1))
      (node (ref U1) (pin 18))
      (node (ref U9) (pin 48))
      (node (ref MCU_PORT1) (pin 21)))
    (net (code 10) (name /QSPI_CS0)
      (node (ref MCU_PORT1) (pin 23))
      (node (ref PULUPEN1) (pin 3))
      (node (ref MCU_PORT1) (pin 23))
      (node (ref U1) (pin 20)))
    (net (code 11) (name /QSPI_CS2)
      (node (ref MCU_PORT1) (pin 27))
      (node (ref U9) (pin 45))
      (node (ref U1) (pin 13)))
    (net (code 12) (name /QSPI_CS3)
      (node (ref MCU_PORT1) (pin 29))
      (node (ref U1) (pin 12)))
    (net (code 13) (name GNDA)
      (node (ref MCU_PORT1) (pin 58))
      (node (ref FB1) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref U1) (pin 47))
      (node (ref MCU_PORT1) (pin 56))
      (node (ref C18) (pin 2))
      (node (ref U1) (pin 48)))
    (net (code 14) (name "Net-(L1-Pad1)")
      (node (ref VDDA1) (pin 2))
      (node (ref L1) (pin 1)))
    (net (code 15) (name /VCCA)
      (node (ref MCU_PORT1) (pin 57))
      (node (ref MCU_PORT1) (pin 55))
      (node (ref C16) (pin 1))
      (node (ref U1) (pin 49))
      (node (ref U1) (pin 50))
      (node (ref L1) (pin 2))
      (node (ref C18) (pin 1)))
    (net (code 16) (name /IRQ-7)
      (node (ref MCU_PORT1) (pin 39))
      (node (ref R13) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref U1) (pin 95)))
    (net (code 17) (name /PWM5)
      (node (ref MCU_PORT1) (pin 30))
      (node (ref U1) (pin 60)))
    (net (code 18) (name /PWM1)
      (node (ref U1) (pin 38))
      (node (ref MCU_PORT1) (pin 13)))
    (net (code 19) (name /PWM3)
      (node (ref U1) (pin 33))
      (node (ref MCU_PORT1) (pin 15)))
    (net (code 20) (name /PWM7)
      (node (ref MCU_PORT1) (pin 32))
      (node (ref U1) (pin 63)))
    (net (code 21) (name /DTIN0)
      (node (ref U1) (pin 36))
      (node (ref MCU_PORT1) (pin 34))
      (node (ref U4) (pin 2)))
    (net (code 22) (name /DTIN1)
      (node (ref MCU_PORT1) (pin 36))
      (node (ref U1) (pin 37))
      (node (ref U4) (pin 5)))
    (net (code 23) (name /DTIN2)
      (node (ref MCU_PORT1) (pin 38))
      (node (ref U4) (pin 12))
      (node (ref U1) (pin 31)))
    (net (code 24) (name /DTIN3)
      (node (ref U4) (pin 9))
      (node (ref MCU_PORT1) (pin 40))
      (node (ref U1) (pin 32)))
    (net (code 25) (name /AN6)
      (node (ref U1) (pin 52))
      (node (ref MCU_PORT1) (pin 22)))
    (net (code 26) (name /AN2)
      (node (ref U1) (pin 45))
      (node (ref MCU_PORT1) (pin 14)))
    (net (code 27) (name /AN3)
      (node (ref U1) (pin 46))
      (node (ref MCU_PORT1) (pin 16)))
    (net (code 28) (name /AN4)
      (node (ref U1) (pin 54))
      (node (ref MCU_PORT1) (pin 18)))
    (net (code 29) (name /AN5)
      (node (ref MCU_PORT1) (pin 20))
      (node (ref U1) (pin 53)))
    (net (code 30) (name /AN7)
      (node (ref U1) (pin 51))
      (node (ref MCU_PORT1) (pin 24)))
    (net (code 31) (name /VDDPLL)
      (node (ref L2) (pin 2))
      (node (ref C20) (pin 1))
      (node (ref C21) (pin 1))
      (node (ref U1) (pin 74)))
    (net (code 32) (name /RSTO-)
      (node (ref MCU_PORT1) (pin 4))
      (node (ref R21) (pin 1))
      (node (ref U1) (pin 97)))
    (net (code 33) (name /RSTI-)
      (node (ref R15) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref BDM_PORT1) (pin 7))
      (node (ref U1) (pin 96))
      (node (ref MCU_PORT1) (pin 6)))
    (net (code 34) (name "Net-(R9-Pad1)")
      (node (ref U1) (pin 5))
      (node (ref R9) (pin 1)))
    (net (code 35) (name "Net-(R22-Pad2)")
      (node (ref R22) (pin 2))
      (node (ref RED1) (pin 1)))
    (net (code 36) (name /GPT0)
      (node (ref MCU_PORT1) (pin 49))
      (node (ref U1) (pin 58)))
    (net (code 37) (name /GPT1)
      (node (ref U1) (pin 59))
      (node (ref MCU_PORT1) (pin 50)))
    (net (code 38) (name /GPT2)
      (node (ref MCU_PORT1) (pin 51))
      (node (ref U1) (pin 61)))
    (net (code 39) (name /GPT3)
      (node (ref MCU_PORT1) (pin 52))
      (node (ref U1) (pin 62)))
    (net (code 40) (name "Net-(Q1-Pad2)")
      (node (ref R21) (pin 2))
      (node (ref Q1) (pin 2)))
    (net (code 41) (name "Net-(Q1-Pad3)")
      (node (ref R22) (pin 1))
      (node (ref Q1) (pin 3)))
    (net (code 42) (name /XTAL)
      (node (ref C2) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref Y1) (pin 2))
      (node (ref U1) (pin 72))
      (node (ref U9) (pin 128)))
    (net (code 43) (name /RCON-)
      (node (ref R45) (pin 1))
      (node (ref U1) (pin 21))
      (node (ref MCU_PORT1) (pin 53)))
    (net (code 44) (name /CANRX)
      (node (ref U1) (pin 11))
      (node (ref CAN_EN1) (pin 4))
      (node (ref PULUPEN1) (pin 7))
      (node (ref MCU_PORT1) (pin 28)))
    (net (code 45) (name /CANTX)
      (node (ref CAN_EN1) (pin 1))
      (node (ref PULUPEN1) (pin 5))
      (node (ref U1) (pin 10))
      (node (ref MCU_PORT1) (pin 26)))
    (net (code 46) (name /UCTS2)
      (node (ref UART_EN2) (pin 8))
      (node (ref MCU_PORT1) (pin 48))
      (node (ref U1) (pin 27)))
    (net (code 47) (name /URTS2)
      (node (ref MCU_PORT1) (pin 46))
      (node (ref U1) (pin 30))
      (node (ref UART_EN2) (pin 6)))
    (net (code 48) (name /UCTS1)
      (node (ref MCU_PORT1) (pin 11))
      (node (ref UART_EN1) (pin 8))
      (node (ref U1) (pin 98))
      (node (ref U9) (pin 49))
      (node (ref P3) (pin 1)))
    (net (code 49) (name /URTS1)
      (node (ref P3) (pin 3))
      (node (ref U1) (pin 4))
      (node (ref MCU_PORT1) (pin 9))
      (node (ref U9) (pin 53))
      (node (ref UART_EN1) (pin 6)))
    (net (code 50) (name /UCTS0)
      (node (ref U1) (pin 6))
      (node (ref MCU_PORT1) (pin 44))
      (node (ref UART_EN0) (pin 8)))
    (net (code 51) (name /URTS0)
      (node (ref U1) (pin 9))
      (node (ref UART_EN0) (pin 6))
      (node (ref MCU_PORT1) (pin 42)))
    (net (code 52) (name /URXD2)
      (node (ref U1) (pin 28))
      (node (ref UART_EN2) (pin 4))
      (node (ref MCU_PORT1) (pin 47)))
    (net (code 53) (name /URXD1)
      (node (ref MCU_PORT1) (pin 7))
      (node (ref U1) (pin 100))
      (node (ref UART_EN1) (pin 4)))
    (net (code 54) (name /UTXD2)
      (node (ref U1) (pin 29))
      (node (ref UART_EN2) (pin 2))
      (node (ref MCU_PORT1) (pin 45)))
    (net (code 55) (name "Net-(C15-Pad1)")
      (node (ref C15) (pin 1))
      (node (ref R7) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref R12) (pin 1)))
    (net (code 56) (name /CLKIN/EXTAL)
      (node (ref C1) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref Y1) (pin 1))
      (node (ref U1) (pin 73)))
    (net (code 57) (name /DSCLK)
      (node (ref R18) (pin 2))
      (node (ref BDM_PORT1) (pin 4))
      (node (ref U1) (pin 85)))
    (net (code 58) (name "Net-(R46-Pad1)")
      (node (ref R46) (pin 1))
      (node (ref U1) (pin 64)))
    (net (code 59) (name "Net-(BDM_PORT1-Pad1)")
      (node (ref BDM_PORT1) (pin 1)))
    (net (code 60) (name "Net-(BDM_PORT1-Pad22)")
      (node (ref BDM_PORT1) (pin 22)))
    (net (code 61) (name "Net-(BDM_PORT1-Pad21)")
      (node (ref BDM_PORT1) (pin 21)))
    (net (code 62) (name /DDAT0)
      (node (ref U1) (pin 77))
      (node (ref BDM_PORT1) (pin 19)))
    (net (code 63) (name "Net-(BDM_PORT1-Pad26)")
      (node (ref TA-1) (pin 1))
      (node (ref BDM_PORT1) (pin 26)))
    (net (code 64) (name /BKPT-)
      (node (ref BDM_PORT1) (pin 2))
      (node (ref U1) (pin 76))
      (node (ref R17) (pin 2)))
    (net (code 65) (name /DDAT1)
      (node (ref U1) (pin 78))
      (node (ref BDM_PORT1) (pin 18)))
    (net (code 66) (name /DDAT2)
      (node (ref BDM_PORT1) (pin 17))
      (node (ref U1) (pin 83)))
    (net (code 67) (name /DDAT3)
      (node (ref BDM_PORT1) (pin 16))
      (node (ref U1) (pin 84)))
    (net (code 68) (name /PST0)
      (node (ref U1) (pin 65))
      (node (ref BDM_PORT1) (pin 15)))
    (net (code 69) (name /PST1)
      (node (ref BDM_PORT1) (pin 14))
      (node (ref U1) (pin 66)))
    (net (code 70) (name /PST2)
      (node (ref BDM_PORT1) (pin 13))
      (node (ref U1) (pin 69)))
    (net (code 71) (name /PST3)
      (node (ref U1) (pin 70))
      (node (ref BDM_PORT1) (pin 12)))
    (net (code 72) (name /DSI)
      (node (ref U1) (pin 79))
      (node (ref R19) (pin 2))
      (node (ref BDM_PORT1) (pin 8)))
    (net (code 73) (name /CLKMOD0)
      (node (ref R25) (pin 2))
      (node (ref CLK0) (pin 2))
      (node (ref U1) (pin 40)))
    (net (code 74) (name /CLKMOD1)
      (node (ref CLK1) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref U1) (pin 39)))
    (net (code 75) (name /JTAG_EN)
      (node (ref R16) (pin 2))
      (node (ref BDM_EN1) (pin 2))
      (node (ref U1) (pin 26)))
    (net (code 76) (name /DSO)
      (node (ref U1) (pin 80))
      (node (ref BDM_PORT1) (pin 10))
      (node (ref R20) (pin 2)))
    (net (code 77) (name "Net-(BDM_PORT1-Pad6)")
      (node (ref CT1) (pin 1))
      (node (ref BDM_PORT1) (pin 6)))
    (net (code 78) (name /UTXD1)
      (node (ref MCU_PORT1) (pin 5))
      (node (ref UART_EN1) (pin 2))
      (node (ref U1) (pin 99)))
    (net (code 79) (name "Net-(C3-Pad1)")
      (node (ref RST_SW1) (pin 1))
      (node (ref LV1) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref D3) (pin 1)))
    (net (code 80) (name /TCLK)
      (node (ref CLKOUT1) (pin 1))
      (node (ref BDM_PORT1) (pin 24))
      (node (ref CT1) (pin 2))
      (node (ref R26) (pin 1))
      (node (ref R46) (pin 2)))
    (net (code 81) (name /URXD0)
      (node (ref MCU_PORT1) (pin 43))
      (node (ref UART_EN0) (pin 4))
      (node (ref U1) (pin 7)))
    (net (code 82) (name /UTXD0)
      (node (ref U1) (pin 8))
      (node (ref UART_EN0) (pin 2))
      (node (ref MCU_PORT1) (pin 41)))
    (net (code 83) (name /ALLPST)
      (node (ref U1) (pin 86))
      (node (ref ALLPST1) (pin 1)))
    (net (code 84) (name "Net-(U8-Pad12)")
      (node (ref U8) (pin 12))
      (node (ref UART_EN2) (pin 7)))
    (net (code 85) (name /inout_user/CAN_L)
      (node (ref R38) (pin 1))
      (node (ref RCAN1) (pin 2))
      (node (ref U7) (pin 6))
      (node (ref COM_SEL3) (pin 1)))
    (net (code 86) (name "Net-(R23-Pad2)")
      (node (ref R23) (pin 2))
      (node (ref U8) (pin 11))
      (node (ref UART_EN2) (pin 5)))
    (net (code 87) (name "Net-(C45-Pad1)")
      (node (ref C45) (pin 1))
      (node (ref U8) (pin 6)))
    (net (code 88) (name "Net-(C36-Pad2)")
      (node (ref C36) (pin 2))
      (node (ref U8) (pin 5)))
    (net (code 89) (name "Net-(C44-Pad2)")
      (node (ref C44) (pin 2))
      (node (ref U8) (pin 3)))
    (net (code 90) (name "Net-(C35-Pad2)")
      (node (ref C35) (pin 2))
      (node (ref U8) (pin 2)))
    (net (code 91) (name /inout_user/TxD_CAN)
      (node (ref U7) (pin 1))
      (node (ref CAN_EN1) (pin 3)))
    (net (code 92) (name "Net-(R36-Pad1)")
      (node (ref RS1) (pin 1))
      (node (ref R36) (pin 1))
      (node (ref U7) (pin 8)))
    (net (code 93) (name "Net-(COM_SEL1-Pad3)")
      (node (ref U8) (pin 13))
      (node (ref COM_SEL1) (pin 3)))
    (net (code 94) (name "Net-(PULUPEN1-Pad8)")
      (node (ref PULUPEN1) (pin 8))
      (node (ref R47) (pin 2)))
    (net (code 95) (name "Net-(PULUPEN1-Pad4)")
      (node (ref PULUPEN1) (pin 4))
      (node (ref R49) (pin 2)))
    (net (code 96) (name "Net-(C32-Pad1)")
      (node (ref U5) (pin 4))
      (node (ref C32) (pin 1)))
    (net (code 97) (name "Net-(C31-Pad1)")
      (node (ref U5) (pin 1))
      (node (ref C31) (pin 1)))
    (net (code 98) (name "Net-(UARTCAN1-Pad1)")
      (node (ref UARTCAN1) (pin 6))
      (node (ref UARTCAN1) (pin 4))
      (node (ref UARTCAN1) (pin 1)))
    (net (code 99) (name "Net-(C27-Pad1)")
      (node (ref C27) (pin 1))
      (node (ref U3) (pin 6)))
    (net (code 100) (name "Net-(C25-Pad2)")
      (node (ref U3) (pin 5))
      (node (ref C25) (pin 2)))
    (net (code 101) (name "Net-(C24-Pad2)")
      (node (ref C24) (pin 2))
      (node (ref U3) (pin 3)))
    (net (code 102) (name "Net-(C23-Pad2)")
      (node (ref C23) (pin 2))
      (node (ref U3) (pin 2)))
    (net (code 103) (name "Net-(C44-Pad1)")
      (node (ref U8) (pin 1))
      (node (ref C44) (pin 1)))
    (net (code 104) (name "Net-(C36-Pad1)")
      (node (ref C36) (pin 1))
      (node (ref U8) (pin 4)))
    (net (code 105) (name "Net-(UARTCAN2-Pad1)")
      (node (ref UARTCAN2) (pin 6))
      (node (ref UARTCAN2) (pin 4))
      (node (ref UARTCAN2) (pin 1)))
    (net (code 106) (name "Net-(C33-Pad1)")
      (node (ref C33) (pin 1))
      (node (ref U5) (pin 6)))
    (net (code 107) (name "Net-(C32-Pad2)")
      (node (ref C32) (pin 2))
      (node (ref U5) (pin 5)))
    (net (code 108) (name "Net-(C31-Pad2)")
      (node (ref U5) (pin 3))
      (node (ref C31) (pin 2)))
    (net (code 109) (name "Net-(C30-Pad2)")
      (node (ref C30) (pin 2))
      (node (ref U5) (pin 2)))
    (net (code 110) (name "Net-(U5-Pad12)")
      (node (ref UART_EN1) (pin 3))
      (node (ref U5) (pin 12)))
    (net (code 111) (name "Net-(U5-Pad9)")
      (node (ref UART_EN1) (pin 7))
      (node (ref U5) (pin 9)))
    (net (code 112) (name "Net-(U5-Pad11)")
      (node (ref UART_EN1) (pin 1))
      (node (ref U5) (pin 11)))
    (net (code 113) (name "Net-(R35-Pad2)")
      (node (ref UART_EN1) (pin 5))
      (node (ref U5) (pin 10))
      (node (ref R35) (pin 2)))
    (net (code 114) (name "Net-(C43-Pad2)")
      (node (ref MCU_PORT1) (pin 1))
      (node (ref C43) (pin 2))
      (node (ref VX_EN1) (pin 2)))
    (net (code 115) (name "Net-(U7-Pad5)")
      (node (ref U7) (pin 5))
      (node (ref VREF1) (pin 1)))
    (net (code 116) (name /inout_user/RxD_CAN)
      (node (ref CAN_EN1) (pin 2))
      (node (ref U7) (pin 4)))
    (net (code 117) (name "Net-(LED_EN1-Pad2)")
      (node (ref U4) (pin 1))
      (node (ref R34) (pin 2))
      (node (ref U4) (pin 4))
      (node (ref U4) (pin 13))
      (node (ref U4) (pin 10))
      (node (ref LED_EN1) (pin 2)))
    (net (code 118) (name "Net-(J1-Pad3)")
      (node (ref SW_ONOFF1) (pin 3))
      (node (ref TB1) (pin 1))
      (node (ref J1) (pin 3)))
    (net (code 119) (name "Net-(F1-Pad1)")
      (node (ref F1) (pin 1))
      (node (ref SW_ONOFF1) (pin 2)))
    (net (code 120) (name "Net-(C38-Pad1)")
      (node (ref F1) (pin 2))
      (node (ref C38) (pin 1))
      (node (ref D7) (pin 1))
      (node (ref VR1) (pin 5))
      (node (ref C41) (pin 1)))
    (net (code 121) (name "Net-(U3-Pad12)")
      (node (ref U3) (pin 12))
      (node (ref UART_EN0) (pin 3)))
    (net (code 122) (name "Net-(U3-Pad9)")
      (node (ref UART_EN0) (pin 7))
      (node (ref U3) (pin 9)))
    (net (code 123) (name "Net-(U3-Pad11)")
      (node (ref U3) (pin 11))
      (node (ref UART_EN0) (pin 1)))
    (net (code 124) (name "Net-(COM_SEL3-Pad3)")
      (node (ref U8) (pin 7))
      (node (ref COM_SEL3) (pin 3)))
    (net (code 125) (name "Net-(U8-Pad10)")
      (node (ref U8) (pin 10))
      (node (ref UART_EN2) (pin 1)))
    (net (code 126) (name "Net-(U8-Pad9)")
      (node (ref UART_EN2) (pin 3))
      (node (ref U8) (pin 9)))
    (net (code 127) (name "Net-(COM_SEL2-Pad3)")
      (node (ref U8) (pin 8))
      (node (ref COM_SEL2) (pin 3)))
    (net (code 128) (name "Net-(PULUPEN1-Pad2)")
      (node (ref PULUPEN1) (pin 2))
      (node (ref R50) (pin 2)))
    (net (code 129) (name "Net-(PULUPEN1-Pad6)")
      (node (ref PULUPEN1) (pin 6))
      (node (ref R48) (pin 2)))
    (net (code 130) (name "Net-(R30-Pad2)")
      (node (ref UART_EN0) (pin 5))
      (node (ref R30) (pin 2))
      (node (ref U3) (pin 10)))
    (net (code 131) (name "Net-(C24-Pad1)")
      (node (ref C24) (pin 1))
      (node (ref U3) (pin 1)))
    (net (code 132) (name "Net-(C25-Pad1)")
      (node (ref U3) (pin 4))
      (node (ref C25) (pin 1)))
    (net (code 133) (name "Net-(UARTCAN0-Pad1)")
      (node (ref UARTCAN0) (pin 4))
      (node (ref UARTCAN0) (pin 1))
      (node (ref UARTCAN0) (pin 6)))
    (net (code 134) (name /inout_user/CAN_H)
      (node (ref CAN_TERM1) (pin 1))
      (node (ref COM_SEL1) (pin 1))
      (node (ref U7) (pin 7))
      (node (ref RCAN2) (pin 2)))
    (net (code 135) (name "Net-(UARTCAN2-Pad9)")
      (node (ref UARTCAN2) (pin 9)))
    (net (code 136) (name /inout_user/RXD2)
      (node (ref COM_SEL2) (pin 2))
      (node (ref UARTCAN2) (pin 3)))
    (net (code 137) (name /inout_user/CTS2/CANH)
      (node (ref COM_SEL1) (pin 2))
      (node (ref UARTCAN2) (pin 7)))
    (net (code 138) (name /inout_user/RTS2)
      (node (ref UARTCAN2) (pin 8))
      (node (ref U8) (pin 14)))
    (net (code 139) (name /inout_user/TXD2/CANL)
      (node (ref COM_SEL3) (pin 2))
      (node (ref UARTCAN2) (pin 2)))
    (net (code 140) (name "Net-(CAN_TERM1-Pad2)")
      (node (ref R38) (pin 2))
      (node (ref CAN_TERM1) (pin 2)))
    (net (code 141) (name "Net-(VR1-Pad4)")
      (node (ref VR1) (pin 4)))
    (net (code 142) (name "Net-(LED5-Pad1)")
      (node (ref LED5) (pin 1))
      (node (ref R53) (pin 1)))
    (net (code 143) (name "Net-(SW_ONOFF1-Pad1)")
      (node (ref SW_ONOFF1) (pin 1)))
    (net (code 144) (name "Net-(R32-Pad2)")
      (node (ref R32) (pin 2))
      (node (ref U4) (pin 11)))
    (net (code 145) (name "Net-(LED4-Pad1)")
      (node (ref LED4) (pin 1))
      (node (ref R33) (pin 1)))
    (net (code 146) (name "Net-(LED3-Pad1)")
      (node (ref LED3) (pin 1))
      (node (ref R32) (pin 1)))
    (net (code 147) (name "Net-(LED2-Pad1)")
      (node (ref LED2) (pin 1))
      (node (ref R31) (pin 1)))
    (net (code 148) (name "Net-(LED1-Pad1)")
      (node (ref R28) (pin 1))
      (node (ref LED1) (pin 1)))
    (net (code 149) (name "Net-(R33-Pad2)")
      (node (ref U4) (pin 8))
      (node (ref R33) (pin 2)))
    (net (code 150) (name "Net-(R31-Pad2)")
      (node (ref R31) (pin 2))
      (node (ref U4) (pin 6)))
    (net (code 151) (name "Net-(R28-Pad2)")
      (node (ref U4) (pin 3))
      (node (ref R28) (pin 2)))
    (net (code 152) (name "Net-(UARTCAN1-Pad9)")
      (node (ref UARTCAN1) (pin 9)))
    (net (code 153) (name /inout_user/CTS1)
      (node (ref U5) (pin 8))
      (node (ref UARTCAN1) (pin 7)))
    (net (code 154) (name /inout_user/RTS1)
      (node (ref U5) (pin 7))
      (node (ref UARTCAN1) (pin 8)))
    (net (code 155) (name /inout_user/RXD1)
      (node (ref UARTCAN1) (pin 3))
      (node (ref U5) (pin 13)))
    (net (code 156) (name /inout_user/TXD1)
      (node (ref U5) (pin 14))
      (node (ref UARTCAN1) (pin 2)))
    (net (code 157) (name "Net-(UARTCAN0-Pad9)")
      (node (ref UARTCAN0) (pin 9)))
    (net (code 158) (name /inout_user/TXD0)
      (node (ref U3) (pin 14))
      (node (ref UARTCAN0) (pin 2)))
    (net (code 159) (name /inout_user/RXD0)
      (node (ref UARTCAN0) (pin 3))
      (node (ref U3) (pin 13)))
    (net (code 160) (name /inout_user/RTS0)
      (node (ref U3) (pin 7))
      (node (ref UARTCAN0) (pin 8)))
    (net (code 161) (name /inout_user/CTS0)
      (node (ref U3) (pin 8))
      (node (ref UARTCAN0) (pin 7)))
    (net (code 162) (name "Net-(U9-Pad9)")
      (node (ref U9) (pin 9)))
    (net (code 163) (name "Net-(U9-Pad90)")
      (node (ref U9) (pin 90)))
    (net (code 164) (name "Net-(U9-Pad91)")
      (node (ref U9) (pin 91)))
    (net (code 165) (name "Net-(U9-Pad92)")
      (node (ref U9) (pin 92)))
    (net (code 166) (name "Net-(U9-Pad93)")
      (node (ref U9) (pin 93)))
    (net (code 167) (name "Net-(U9-Pad94)")
      (node (ref U9) (pin 94)))
    (net (code 168) (name /xilinx/XIL_D5)
      (node (ref U9) (pin 143))
      (node (ref P4) (pin 11)))
    (net (code 169) (name /xilinx/XIL_D4)
      (node (ref P4) (pin 9))
      (node (ref U9) (pin 2)))
    (net (code 170) (name /xilinx/XIL_D1)
      (node (ref U9) (pin 11))
      (node (ref P4) (pin 3)))
    (net (code 171) (name /xilinx/XIL_D0)
      (node (ref U9) (pin 12))
      (node (ref P4) (pin 1)))
    (net (code 172) (name "Net-(U9-Pad55)")
      (node (ref U9) (pin 55)))
    (net (code 173) (name "Net-(U9-Pad56)")
      (node (ref U9) (pin 56)))
    (net (code 174) (name "Net-(U9-Pad29)")
      (node (ref U9) (pin 29)))
    (net (code 175) (name "Net-(U9-Pad30)")
      (node (ref U9) (pin 30)))
    (net (code 176) (name "Net-(P3-Pad4)")
      (node (ref P3) (pin 4))
      (node (ref U9) (pin 31)))
    (net (code 177) (name "Net-(U9-Pad34)")
      (node (ref U9) (pin 34)))
    (net (code 178) (name "Net-(U9-Pad35)")
      (node (ref U9) (pin 35)))
    (net (code 179) (name "Net-(U9-Pad36)")
      (node (ref U9) (pin 36)))
    (net (code 180) (name "Net-(U9-Pad37)")
      (node (ref U9) (pin 37)))
    (net (code 181) (name "Net-(U9-Pad38)")
      (node (ref U9) (pin 38)))
    (net (code 182) (name "Net-(U9-Pad39)")
      (node (ref U9) (pin 39)))
    (net (code 183) (name "Net-(U9-Pad40)")
      (node (ref U9) (pin 40)))
    (net (code 184) (name "Net-(U9-Pad41)")
      (node (ref U9) (pin 41)))
    (net (code 185) (name "Net-(U9-Pad80)")
      (node (ref U9) (pin 80)))
    (net (code 186) (name "Net-(U9-Pad74)")
      (node (ref U9) (pin 74)))
    (net (code 187) (name "Net-(U9-Pad75)")
      (node (ref U9) (pin 75)))
    (net (code 188) (name "Net-(U9-Pad77)")
      (node (ref U9) (pin 77)))
    (net (code 189) (name "Net-(U9-Pad78)")
      (node (ref U9) (pin 78)))
    (net (code 190) (name "Net-(U9-Pad79)")
      (node (ref U9) (pin 79)))
    (net (code 191) (name /xilinx/XIL_D3)
      (node (ref P4) (pin 7))
      (node (ref U9) (pin 8)))
    (net (code 192) (name "Net-(U9-Pad81)")
      (node (ref U9) (pin 81)))
    (net (code 193) (name "Net-(U9-Pad82)")
      (node (ref U9) (pin 82)))
    (net (code 194) (name "Net-(U9-Pad83)")
      (node (ref U9) (pin 83)))
    (net (code 195) (name "Net-(U9-Pad84)")
      (node (ref U9) (pin 84)))
    (net (code 196) (name "Net-(U9-Pad86)")
      (node (ref U9) (pin 86)))
    (net (code 197) (name "Net-(U9-Pad87)")
      (node (ref U9) (pin 87)))
    (net (code 198) (name "Net-(U9-Pad88)")
      (node (ref U9) (pin 88)))
    (net (code 199) (name "Net-(U9-Pad60)")
      (node (ref U9) (pin 60)))
    (net (code 200) (name "Net-(U9-Pad61)")
      (node (ref U9) (pin 61)))
    (net (code 201) (name "Net-(U9-Pad62)")
      (node (ref U9) (pin 62)))
    (net (code 202) (name "Net-(U9-Pad63)")
      (node (ref U9) (pin 63)))
    (net (code 203) (name "Net-(U9-Pad65)")
      (node (ref U9) (pin 65)))
    (net (code 204) (name "Net-(U9-Pad66)")
      (node (ref U9) (pin 66)))
    (net (code 205) (name "Net-(U9-Pad67)")
      (node (ref U9) (pin 67)))
    (net (code 206) (name "Net-(U9-Pad68)")
      (node (ref U9) (pin 68)))
    (net (code 207) (name "Net-(U9-Pad69)")
      (node (ref U9) (pin 69)))
    (net (code 208) (name /xilinx/XIL_D2)
      (node (ref U9) (pin 7))
      (node (ref P4) (pin 5)))
    (net (code 209) (name "Net-(U9-Pad70)")
      (node (ref U9) (pin 70)))
    (net (code 210) (name "Net-(U9-Pad71)")
      (node (ref U9) (pin 71)))
    (net (code 211) (name "Net-(U9-Pad72)")
      (node (ref U9) (pin 72)))
    (net (code 212) (name /xilinx/LED_TEST2)
      (node (ref U9) (pin 27))
      (node (ref R63) (pin 1)))
    (net (code 213) (name "Net-(D9-Pad1)")
      (node (ref D9) (pin 1))
      (node (ref R63) (pin 2)))
    (net (code 214) (name /xilinx/TMS)
      (node (ref P1) (pin 3))
      (node (ref U9) (pin 20)))
    (net (code 215) (name /xilinx/TDI)
      (node (ref U9) (pin 4))
      (node (ref P1) (pin 4)))
    (net (code 216) (name /xilinx/TDO)
      (node (ref U9) (pin 104))
      (node (ref P1) (pin 6)))
    (net (code 217) (name /xilinx/XIL_D14)
      (node (ref U9) (pin 109))
      (node (ref P4) (pin 29)))
    (net (code 218) (name /xilinx/XIL_D28)
      (node (ref U9) (pin 132))
      (node (ref P4) (pin 20)))
    (net (code 219) (name /xilinx/XIL_D10)
      (node (ref P4) (pin 21))
      (node (ref U9) (pin 122)))
    (net (code 220) (name /xilinx/XIL_D29)
      (node (ref U9) (pin 117))
      (node (ref P4) (pin 22)))
    (net (code 221) (name /xilinx/XIL_D11)
      (node (ref U9) (pin 119))
      (node (ref P4) (pin 23)))
    (net (code 222) (name /xilinx/XIL_D30)
      (node (ref P4) (pin 24))
      (node (ref U9) (pin 118)))
    (net (code 223) (name /xilinx/XIL_D12)
      (node (ref P4) (pin 25))
      (node (ref U9) (pin 114)))
    (net (code 224) (name /xilinx/XIL_D31)
      (node (ref P4) (pin 26))
      (node (ref U9) (pin 116)))
    (net (code 225) (name /xilinx/XIL_D13)
      (node (ref U9) (pin 111))
      (node (ref P4) (pin 27)))
    (net (code 226) (name /xilinx/XIL_D32)
      (node (ref P4) (pin 28))
      (node (ref U9) (pin 98)))
    (net (code 227) (name /xilinx/XIL_D9)
      (node (ref U9) (pin 131))
      (node (ref P4) (pin 19)))
    (net (code 228) (name /xilinx/XIL_D33)
      (node (ref U9) (pin 112))
      (node (ref P4) (pin 30)))
    (net (code 229) (name /xilinx/XIL_D15)
      (node (ref P4) (pin 31))
      (node (ref U9) (pin 108)))
    (net (code 230) (name /xilinx/XIL_D34)
      (node (ref U9) (pin 113))
      (node (ref P4) (pin 32)))
    (net (code 231) (name /xilinx/XIL_D16)
      (node (ref P4) (pin 33))
      (node (ref U9) (pin 100)))
    (net (code 232) (name /xilinx/XIL_D35)
      (node (ref P4) (pin 34))
      (node (ref U9) (pin 107)))
    (net (code 233) (name /xilinx/XIL_D17)
      (node (ref P4) (pin 35))
      (node (ref U9) (pin 101)))
    (net (code 234) (name /xilinx/XIL_D36)
      (node (ref U9) (pin 99))
      (node (ref P4) (pin 36)))
    (net (code 235) (name /xilinx/XIL_D18)
      (node (ref U9) (pin 97))
      (node (ref P4) (pin 37)))
    (net (code 236) (name /xilinx/+3,3V_OUT)
      (node (ref P4) (pin 38))
      (node (ref R64) (pin 2)))
    (net (code 237) (name /xilinx/XIL_D23)
      (node (ref U9) (pin 1))
      (node (ref P4) (pin 10)))
    (net (code 238) (name /xilinx/XIL_D24)
      (node (ref U9) (pin 142))
      (node (ref P4) (pin 12)))
    (net (code 239) (name /xilinx/XIL_D6)
      (node (ref U9) (pin 140))
      (node (ref P4) (pin 13)))
    (net (code 240) (name /xilinx/XIL_D25)
      (node (ref P4) (pin 14))
      (node (ref U9) (pin 139)))
    (net (code 241) (name /xilinx/XIL_D7)
      (node (ref P4) (pin 15))
      (node (ref U9) (pin 138)))
    (net (code 242) (name /xilinx/XIL_D26)
      (node (ref U9) (pin 137))
      (node (ref P4) (pin 16)))
    (net (code 243) (name /xilinx/XIL_D8)
      (node (ref U9) (pin 136))
      (node (ref P4) (pin 17)))
    (net (code 244) (name /xilinx/XIL_D27)
      (node (ref U9) (pin 134))
      (node (ref P4) (pin 18)))
    (net (code 245) (name /xilinx/TCK)
      (node (ref R57) (pin 2))
      (node (ref P1) (pin 5))
      (node (ref U9) (pin 89)))
    (net (code 246) (name /xilinx/LED_TEST1)
      (node (ref U9) (pin 28))
      (node (ref R62) (pin 1)))
    (net (code 247) (name "Net-(D8-Pad1)")
      (node (ref R62) (pin 2))
      (node (ref D8) (pin 1)))
    (net (code 248) (name /xilinx/XIL_D19)
      (node (ref U9) (pin 96))
      (node (ref P4) (pin 39)))
    (net (code 249) (name /xilinx/XIL_D20)
      (node (ref P4) (pin 4))
      (node (ref U9) (pin 6)))
    (net (code 250) (name /xilinx/XIL_D21)
      (node (ref P4) (pin 6))
      (node (ref U9) (pin 10)))
    (net (code 251) (name /xilinx/XIL_D22)
      (node (ref P4) (pin 8))
      (node (ref U9) (pin 5)))
    (net (code 252) (name "Net-(U9-Pad110)")
      (node (ref U9) (pin 110)))
    (net (code 253) (name "Net-(U9-Pad102)")
      (node (ref U9) (pin 102)))
    (net (code 254) (name "Net-(U9-Pad103)")
      (node (ref U9) (pin 103)))
    (net (code 255) (name "Net-(U9-Pad106)")
      (node (ref U9) (pin 106)))
    (net (code 256) (name "Net-(U9-Pad121)")
      (node (ref U9) (pin 121)))
    (net (code 257) (name "Net-(U9-Pad120)")
      (node (ref U9) (pin 120)))
    (net (code 258) (name "Net-(U9-Pad141)")
      (node (ref U9) (pin 141)))
    (net (code 259) (name "Net-(U9-Pad133)")
      (node (ref U9) (pin 133)))
    (net (code 260) (name "Net-(U9-Pad25)")
      (node (ref U9) (pin 25)))
    (net (code 261) (name "Net-(P3-Pad2)")
      (node (ref P3) (pin 2))
      (node (ref U9) (pin 32)))
    (net (code 262) (name "Net-(U9-Pad18)")
      (node (ref U9) (pin 18)))
    (net (code 263) (name "Net-(U9-Pad15)")
      (node (ref U9) (pin 15)))
    (net (code 264) (name "Net-(U9-Pad16)")
      (node (ref U9) (pin 16)))
    (net (code 265) (name "Net-(U9-Pad19)")
      (node (ref U9) (pin 19)))
    (net (code 266) (name "Net-(U9-Pad21)")
      (node (ref U9) (pin 21)))
    (net (code 267) (name "Net-(U9-Pad22)")
      (node (ref U9) (pin 22)))
    (net (code 268) (name "Net-(U9-Pad23)")
      (node (ref U9) (pin 23)))
    (net (code 269) (name "Net-(U9-Pad14)")
      (node (ref U9) (pin 14)))
    (net (code 270) (name "Net-(U9-Pad26)")
      (node (ref U9) (pin 26)))
    (net (code 271) (name /AN0)
      (node (ref MCU_PORT1) (pin 10))
      (node (ref U1) (pin 43)))
    (net (code 272) (name /AN1)
      (node (ref U1) (pin 44))
      (node (ref MCU_PORT1) (pin 12)))
    (net (code 273) (name /IRQ-6)
      (node (ref R11) (pin 1))
      (node (ref U1) (pin 94))
      (node (ref MCU_PORT1) (pin 37)))
    (net (code 274) (name /IRQ-5)
      (node (ref R10) (pin 1))
      (node (ref SW2) (pin 1))
      (node (ref MCU_PORT1) (pin 35))
      (node (ref U1) (pin 91)))
    (net (code 275) (name /IRQ-4)
      (node (ref R8) (pin 1))
      (node (ref SW1) (pin 1))
      (node (ref MCU_PORT1) (pin 33))
      (node (ref U1) (pin 90)))
    (net (code 276) (name /IRQ-3)
      (node (ref U9) (pin 44))
      (node (ref U1) (pin 89))
      (node (ref MCU_PORT1) (pin 31))
      (node (ref R6) (pin 1)))
    (net (code 277) (name /IRQ-2)
      (node (ref MCU_PORT1) (pin 8))
      (node (ref U1) (pin 88))
      (node (ref U9) (pin 43))
      (node (ref R5) (pin 1)))
    (net (code 278) (name /IRQ-1)
      (node (ref MCU_PORT1) (pin 2))
      (node (ref U1) (pin 87))
      (node (ref U9) (pin 42))
      (node (ref R4) (pin 1)))))